GSIC - Global Service Information Center

# CYLINDER HEAD > DISASSEMBLY

## for Preparation Click here

HINT:

1. Thoroughly clean all parts to be assembled.
2. Before installing the parts, apply fresh engine oil to all sliding and rotating surfaces.
3. Replace all gaskets and oil seals with new ones.

1. REMOVE VALVE LIFTER

1. Remove the valve lifter.

   HINT:
     Arrange the valve lifters in the correct order.

2. REMOVE INTAKE VALVE

1. Using SST, compress the compression spring and remove the 2 keepers.

   SST
     09202-70020 (09202-00020)

1. Remove the spring retainer, compression spring, valve and spring seat.

   HINT:
     Arrange the valves, compression springs, spring seats and spring retainers in the correct order.

3. REMOVE EXHAUST VALVE

1. Using SST, compress the compression spring and remove the 2 keepers.

   SST
     09202-70020 (09202-00020)

1. Remove the spring retainer, compression spring, valve and spring seat.

   HINT:
     Arrange the valves, compression springs, spring seats and spring retainers in the correct order.

4. REMOVE SEMICIRCULAR PLUG