GSIC - Global Service Information Center

# REAR SPEAKER (for Extra Cab) > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the RH side and LH side.
2. The procedures listed below are for the LH side.

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE BACK PANEL GARNISH UPPER

1. Using a screwdriver, detach the 4 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 5 clips and remove the garnish.

3. REMOVE REAR SEAT CUSHION ASSEMBLY LH

1. Pull the seat cushion lock hook's release lever in the direction of the arrow, and then disconnect the hook on the front of the seat cushion.

1. Detach the seat cushion's 2 rear hooks from the vehicle body.

1. Remove the seat cushion.

4. REMOVE REAR SEAT CUSHION ASSEMBLY RH

HINT:

  Use the same procedures described for the LH side.

5. REMOVE BACK PANEL GARNISH LOWER

1. Using a screwdriver, detach the 6 claws.

   HINT:
     Tape the screwdriver tip before use.

1. Using a clip remover, detach the 5 clips and remove the garnish.

6. REMOVE REAR SEATBACK ASSEMBLY

1. Remove the 2 bolts.

1. Lift up the seatback in the direction indicated by the arrow in the illustration to detach the 2 hooks from the vehicle body. Then remove the seatback.

   NOTICE:
     Be careful not to damage the vehicle body.

7. REMOVE FRONT SEAT OUTER BELT ASSEMBLY LH

1. Single cab:
   Remove the outer belt shoulder anchor.

   1. Using a screwdriver, detach the 2 claws and open the seat belt anchor cover.

      HINT:
        Tape the screwdriver tip before use.

   2. Remove the bolt and shoulder anchor.

1. Double cab:
   Remove the outer belt shoulder anchor.

   1. Using a screwdriver, disengage the 4 claws and remove the seat belt anchor cover cap.

      HINT:
        Tape the screwdriver tip before use.

   2. Remove the bolt and shoulder anchor.

1. w/o Pretensioner:
   Remove the bolt and seat belt.

1. w/ Pretensioner:

   1. Disconnect the pretensioner connector as shown in the illustration.

   2. Remove the bolt and seat belt.

8. REMOVE REAR NO. 1 SEAT BELT ASSEMBLY OUTER LH

1. Remove the bolt and floor anchor.

1. Using a screwdriver, detach the 2 claws and open the seat belt anchor cover.

   HINT:
     Tape the screwdriver tip before use.

1. Remove the bolt.

1. Remove the bolt and seat belt.

9. REMOVE QUARTER INSIDE TRIM BOARD

1. Using a clip remover, detach the 7 clips.

1. Using a screwdriver, detach the 6 claws and remove the trim board.

   HINT:
     Tape the screwdriver tip before use.

1. Detach the claws and remove the trim pocket from the trim board.

10. REMOVE REAR NO. 1 SPEAKER ASSEMBLY

1. Disconnect the connector.

1. Remove the 3 screws and speaker.