GSIC - Global Service Information Center

# REAR SEAT ASSEMBLY (for Double Cab) > INSTALLATION

## for Preparation Click here

1. INSTALL REAR SEAT ASSEMBLY

1. Place the seat in the cabin.

   NOTICE:
     Be careful not to damage the vehicle body.

1. Attach the seatback's 2 hooks to the vehicle body.

1. Install the seat with the 4 bolts.

   Torque:
     19.5 N*m{ 199 kgf*cm , 14 ft.*lbf }

   HINT:
     Tighten the bolts in the order indicated in the illustration.

1. Pass the inner belts between the seat cushion and seatback.

1. Fold down the seat cushion.

1. Hook the fold seat stopper band around the knob.

2. INSTALL REAR SEAT HINGE COVER LH

1. Attach the 3 claws to install the hinge cover.

3. INSTALL REAR SEAT HINGE COVER RH

HINT:

  Use the same procedures described for the LH side.