GSIC - Global Service Information Center

# INTEGRATION RELAY > ON-VEHICLE INSPECTION

## for Preparation Click here

1. CHECK INTEGRATION RELAY

1. Using a screwdriver, detach the 2 claws and disconnect the integration relay from the engine room junction block.

   HINT:
     Tape the screwdriver tip before use.

   1. Measure the voltage of the C/OPN relay.

      Standard resistance:

        Tester Connection | Condition | Specified Condition
        IJ-8 - Body ground | Ignition switch ON | 10 to 14 V

      If the result is not as specified, replace the integration relay.

   2. Measure the voltage of the MAIN relay.

      Standard resistance:

        Tester Connection | Condition | Specified Condition
        IJ-4 - Body ground | Ignition switch ON | 10 to 14 V

      If the result is not as specified, replace the integration relay.