GSIC - Global Service Information Center

# CANISTER > INSPECTION

## for Preparation Click here

1. INSPECT CANISTER ASSEMBLY

1. Inspect operation of the canister.

   Standard operation:

     Condition | Specified Condition
     Close port B and C, then apply vacuum to port A | No leak
     Close port C, then blow air into port A | Air flows from B
     Blow air into port A | Air flows from both port B and C

   If the result is not as specified, replace the canister assembly.