GSIC - Global Service Information Center

# FRONT PROPELLER SHAFT ASSEMBLY > REMOVAL

## for Preparation Click here

1. REMOVE FRONT PROPELLER SHAFT ASSEMBLY

1. Place matchmarks on the propeller shaft flange and differential.

1. Remove the 4 nuts, 4 bolts and 4 washers, and disconnect the propeller shaft.

1. Place matchmarks on the propeller shaft flange and transfer flange.

1. Remove the 4 nuts, 4 washers and front propeller shaft.

2. INSPECT FRONT PROPELLER SHAFT ASSEMBLY

1. Using a dial indicator, measure the propeller shaft runout.

   Maximum runout:
     0.3 mm (0.0120 in.)
   If the shaft runout is greater than the maximum, replace the propeller shaft.

3. INSPECT UNIVERSAL JOINT SPIDER ASSEMBLY

1. Check the spider bearings for wear or damage.

1. Check each spider bearing's axial play by turning the yoke while holding the shaft tightly.

   Maximum bearing axial play:
     0.05 mm (0.0020 in.)
   If the bearing axial play is greater than the maximum, replace the spider bearing.