GSIC - Global Service Information Center

# METER / GAUGE SYSTEM > INITIALIZATION

## for Preparation Click here

HINT:

  The procedures described below are for vehicles with a 1KD-FTV or 2KD-FTV engine.

DESCRIPTION

1. T-BELT warning light

   1. The T-BELT warning light turns on when the odometer displays 150,000 km to indicate that the timing belt should be replaced.

2. Fuel system warning light

   1. The fuel system warning light illuminates when a fuel filter clog is detected.

   2. The fuel system warning light blinks when a certain amount of water is accumulated at the bottom of the fuel filter.

RESET T-BELT WARNING LIGHT

1. When the T-BELT warning light illuminates, follow the procedures below to reset the combination meter.

   1. Push and release the trip meter knob to change the meter display ODO mode.

   2. Turn the ignition switch OFF.

   3. Press and hold the knob, and turn the ignition switch ON.

   4. Keep the knob pushed for 5 seconds or more.

   5. Release the knob and then push it again within 5 seconds.

   6. Release the knob.

   7. Push and release the knob to choose the interval before the next warning light illumination.

      HINT:
        If this step is not performed within 30 seconds of the previous step, the warning light illumination interval will not change and the display will return to ODO mode automatically.

   8. After selecting the interval, hold the knob for 5 seconds or more.

   9. The meter display returns to ODO mode and the warning light turns off.

      HINT:
        The interval before the next warning light illumination can be calculated by taking the 2 digit value from the meter display and multiplying it by 10,000. 150,000 km is the default value when the vehicle is shipped.

RESET FUEL SYSTEM WARNING LIGHT

1. When the fuel system warning light blinks, drain accumulated water from the fuel filter assembly.

2. When the fuel system warning light illuminates, follow the procedures below to reset the combination meter.

   1. Replace the fuel filter.

   2. Disconnect the F4 filter warning switch connector.

   3. Turn the ignition switch ON.

   4. Wait 3 seconds.

   5. Reconnect the F4 connector within 57 seconds.

   6. Make sure that the fuel system warning light turns off 3 seconds after the connector is reconnected.