GSIC - Global Service Information Center

# DIESEL THROTTLE BODY > INSTALLATION

## for Preparation Click here

1. INSTALL DIESEL THROTTLE BODY ASSEMBLY

1. Install a new gasket and the throttle body with the 2 bolts and 2 nuts.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf }

1. Connect the 2 connectors.

2. INSTALL CHARGE AIR COOLER ASSEMBLY WITH INTAKE AIR CONNECTOR

1. Install the intake air connector to the air hoses.

1. Install the CAC with the 4 bolts.

   Torque:
     32 N*m{ 326 kgf*cm , 24 ft.*lbf } for bolt A
     12 N*m{ 125 kgf*cm , 9 ft.*lbf } for bolts B, C and D

1. Tighten the 2 clamps.

1. Connect the vacuum hose the the manifold absolute pressure sensor.

1. Connect the IAT sensor connector and manifold absolute diesel pressure sensor connector.

3. INSTALL NO. 1 ENGINE COVER SUB-ASSEMBLY

1. Install the engine cover with the 3 bolts and 2 nuts.

   Torque:
     7.0 N*m{ 71 kgf*cm , 62 in.*lbf }

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.