GSIC - Global Service Information Center

### CHARGING SYSTEM > PRECAUTION

1. Check that the battery cables are connected to the correct terminals.

1. Disconnect the battery cables when the battery is given a quick charge.

1. Do not perform tests with a high voltage insulation resistance tester.

1. Never disconnect the battery while the engine is running.

1. Check that the charging cable nut is tightened on terminal B of the generator and the fuse box.

1. If the generator is installed to the vehicle, do not perform checks on terminal F.