GSIC - Global Service Information Center

# POWER STEERING > TORQUE SPECIFICATIONS

1GR-FE
Part tightened | N*m | kgf*cm | ft.*lbf
Power steering vane pump
Vane pump housing rear x Vane pump housing front | 22 | 224 | 16
Pressure port union | 69 | 704 | 51
Suction port union set bolt | 9.0 | 92 | 80 in.*lbf
Vane pump assembly x Engine | 21 | 214 | 15
Pressure feed tube assembly x Vane pump assembly | 49 | 500 | 36

TR Series Engine
Part tightened | N*m | kgf*cm | ft.*lbf
Power steering vane pump
Vane pump housing rear x Vane pump housing front | 22 | 224 | 16
Pressure port union | 69 | 704 | 51
Pump oil reservoir x Vane pump assembly | 9.0 | 92 | 80 in.*lbf
Vane pump assembly x Engine | 21 | 214 | 16
Pressure feed tube assembly x Vane pump assembly | 49 | 500 | 36

KD Series Engine
Part tightened | N*m | kgf*cm | ft.*lbf
Power steering vane pump
Vane pump housing rear x Vane pump housing front | 22 | 224 | 16
Pressure port union | 69 | 704 | 51
Suction port union set bolt | 22 | 224 | 16
Vane pump assembly x Engine | 39 | 398 | 2.9
Pressure feed tube assembly x Vane pump assembly | 44 (40) | 449 (407) | 33 (54)

1. ( ): For use without SST

Part tightened | N*m | kgf*cm | ft.*lbf
Engine under cover No. 1 Body for 4WD | 28 | 286 | 21
Engine under cover No. 2 x Body for 4WD | 50 | 510 | 37
Power steering link assembly
Control valve housing set bolt | 18.1 | 185 | 13
Rack guide spring cap | 25 | 250 | 18
Rack guide spring cap lock nut | 69 (65) | 700 (660) | 51 (48)
Power steering rack x Rack end | 103 (98) | 1,050 (1,000) | 76 (72)
Tie rod assembly lock nut | 55.5 | 566 | 41
Turn pressure tube union nut | 12.6 (11.9) | 128 (121) | 9 (9)
Power steering link assembly set bolt and nut | 95 | 969 | 70
Pressure feed and return tubes x Control valve housing | 12.5 | 127 | 9
Pressure feed tube clamp set bolt | 28 | 286 | 21
Outlet return tube | 44 | 499 | 33
Tie rod end x steering knuckle | 49 | 500 | 36
Stabilizer bar front bracket set bolt | 48 | 489 | 35

1. ( ): For use without SST