GSIC - Global Service Information Center

# BACK-UP LIGHT SWITCH > INSTALLATION

## for Preparation Click here

1. INSTALL BACK-UP LIGHT SWITCH ASSEMBLY

1. Using SST, install a new gasket and the back-up light switch to the transmission case.

   SST
     09817-16011

2. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

3. PERFORM INITIALIZATION

1. Perform initialization (Click here ).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.