GSIC - Global Service Information Center

# THERMOSTAT > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag activation.

2. REMOVE NO. 1 ENGINE UNDER COVER

1. Remove the 4 bolts and cover.

3. DRAIN ENGINE COOLANT

NOTICE:

  Do not remove the radiator reservoir cap while the engine and radiator are still hot. Pressurized, hot engine coolant and steam may be released and cause serious burns.

1. Drain the coolant by removing the reservoir cap and, using a wrench, remove the vent plug.

1. Loosen the cylinder block drain cock plug and the radiator drain cock plug.

   HINT:
     Collect the coolant in a container and dispose of it according to the regulations in your area.

4. REMOVE AIR CLEANER ASSEMBLY

1. Remove the clamp and disconnect the IAT connector.

1. Loosen the clamp of the turbocharger.

1. Slide the clamp and disconnect the ventilation hose.

1. Remove the 2 bolts and air cleaner.

5. DISCONNECT RADIATOR HOSE INLET

6. REMOVE WATER INLET

1. Remove the 3 bolts and inlet.

7. REMOVE THERMOSTAT