GSIC - Global Service Information Center

# STEERING PAD > INSTALLATION

## for Preparation Click here

CAUTION:

  Be sure to read the precautionary notices concerning the SRS airbag system before servicing (Click here).

1. INSTALL STEERING PAD ASSEMBLY

1. Support the steering pad with one hand as shown in the illustration.

1. Connect the airbag connector.

   NOTICE:
     When handling the airbag connector, do not damage the airbag wire harness.

1. Connect the horn connector.

1. Install the steering pad after confirming that the circumference grooves of the screws are caught on the screw case.

1. Using a T30 "torx" socket, install the 2 screws.

   Torque:
     8.8 N*m{ 90 kgf*cm , 78 in.*lbf }

2. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

3. INSPECT STEERING PAD ASSEMBLY

1. Check for cuts, cracks or discoloration on the steering pad outer surface and in the grooved portion.

1. Check that the horn sounds.

4. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   CAUTION:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

5. INSPECT SRS WARNING LIGHT

1. Check the SRS warning light (Click here).