GSIC - Global Service Information Center

# ELECTRONIC CONTROLLED AUTOMATIC TRANSMISSION SYSTEM > PRECAUTION

## for Preparation Click here

NOTICE:

  When disconnecting the cable from the negative (-) battery terminal, initialize the following system(s) after the cable is reconnected.

System Name | See procedure
Combination Meter | Click here

HINT:

  Initialization cannot be completed by only reconnecting the cable to the negative (-) battery terminal.