GSIC - Global Service Information Center

### FRONT DIFFERENTIAL CARRIER ASSEMBLY > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE FRONT WHEEL

3. REMOVE FRONT SIDE MEMBER TO FRONT SUSPENSION CROSSMEMBER BRACE

4. REMOVE NO. 1 ENGINE UNDER COVER

5. REMOVE NO. 2 ENGINE UNDER COVER

6. DRAIN DIFFERENTIAL OIL

7. REMOVE FRONT PROPELLER SHAFT ASSEMBLY

8. REMOVE FRONT STABILIZER LINK ASSEMBLY LH

9. REMOVE FRONT STABILIZER LINK ASSEMBLY RH

10. REMOVE TIE ROD END SUB-ASSEMBLY LH

11. REMOVE TIE ROD END SUB-ASSEMBLY RH

12. REMOVE NO. 1 FRONT SUSPENSION ARM SUB-ASSEMBLY LOWER LH

13. REMOVE NO. 1 FRONT SUSPENSION ARM SUB-ASSEMBLY LOWER RH

14. DISCONNECT FRONT AXLE ASSEMBLY LH

15. DISCONNECT FRONT AXLE ASSEMBLY RH

16. REMOVE FRONT DRIVE SHAFT ASSEMBLY LH

17. REMOVE FRONT DRIVE SHAFT ASSEMBLY RH

18. REMOVE FRONT DIFFERENTIAL CARRIER ASSEMBLY