GSIC - Global Service Information Center

# TRANSFER CASE OIL SEAL > REMOVAL

## for Preparation Click here

1. DRAIN TRANSFER OIL

2. REMOVE LOWER TRANSFER CASE PROTECTOR

1. Remove the 4 bolts and protector.

3. REMOVE FRONT PROPELLER SHAFT ASSEMBLY

1. Remove the front propeller shaft (Click here).

4. REMOVE OUTPUT SHAFT COMPANION FLANGE SUB-ASSEMBLY

1. Using a chisel and hammer, loosen the staked part of the lock nut.

1. Using SST to hold the companion flange, remove the lock nut.

   SST
     09330-00021

1. Using SST, remove the companion flange.

   SST
     09950-40011 (09951-04020, 09952-04010, 09953-04030, 09954-04010, 09955-04051, 09957-04010, 09958-04011)

5. REMOVE TRANSFER CASE OIL SEAL

1. Using SST, tap out the oil seal.

   SST
     09308-00010

   NOTICE:
     Be careful not to damage the oil seal and case front contact surface.