GSIC - Global Service Information Center

# TRANSFER ADAPTOR OIL SEAL > INSTALLATION

## for Preparation Click here

1. INSTALL TRANSFER ADAPTER OIL SEAL

1. Coat the lip of a new oil seal with MP grease.

1. Using SST and a hammer, tap in the oil seal.

   SST
     09223-00010

   Oil seal depth:
     45.9 +- 0.5 mm (1.807 +- 0.020 in.)

   NOTICE:
     Be careful not to damage the lip of the oil seal.

2. INSTALL TRANSFER ASSEMBLY

1. Install the transfer assembly (Click here).

3. INSTALL MANUAL TRANSMISSION UNIT ASSEMBLY

1. Install the manual transmission unit assembly (Click here).