GSIC - Global Service Information Center

# IGNITION COIL > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

NOTICE:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag activation.

2. REMOVE INTAKE AIR CONNECTOR

1. Disconnect the vacuum hose.

1. Disconnect the No. 2 ventilation hose.

1. Loosen the hose clamp and remove the 2 bolts and intake air connector.

3. REMOVE IGNITION COIL

1. Disconnect the 4 ignition coil connectors.

1. Remove the 4 bolts and pull out the 4 ignition coils.