GSIC - Global Service Information Center

# LOAD SENSING PROPORTIONING VALVE > REMOVAL

## for Preparation Click here

1. DRAIN BRAKE FLUID

NOTICE:

  Wash off brake fluid immediately if it comes in contact with any painted surface.

2. DISCONNECT NO. 2 LOAD SENSING SPRING SHACKLE

1. Remove the bolt, collar and 2 cushions.

1. Disconnect the shackle from the rear differential.

3. REMOVE LOAD SENSING PROPORTIONING VALVE ASSEMBLY

1. Using SST, disconnect the 3 brake lines from the valve body.

   SST
     09023-00101

1. Remove the 3 bolts and valve.