GSIC - Global Service Information Center

# MASS AIR FLOW METER > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE MASS AIR FLOW METER

1. Disconnect the MAF meter connector.

1. Remove the 2 screws and MAF meter.

1. Remove the O-ring from the MAF meter.