GSIC - Global Service Information Center

### DTC P0010/39 Camshaft Position "A" Actuator Circuit (Bank 1)

DESCRIPTION

MONITOR DESCRIPTION

WIRING DIAGRAM

INSPECTION PROCEDURE

When using intelligent tester:

PERFORM ACTIVE TEST (OPERATE OCV)

CHECK CAMSHAFT TIMING OIL CONTROL VALVE ASSEMBLY (OCV SIGNAL)

CHECK ECM (OCV SIGNAL)

When not using intelligent tester:

CHECK CAMSHAFT TIMING CONTROL VALVE ASSEMBLY (OPERATE OCV)

CHECK ECM (OCV SIGNAL)

CHECK WIRE HARNESS (CAMSHAFT TIMING OIL CONTROL VALVE (OCV) - ECM)