GSIC - Global Service Information Center

# BRAKE ACTUATOR > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

NOTICE:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. DRAIN BRAKE FLUID

NOTICE:

  Wash off brake fluid immediately if it comes in contact with any painted surface.

3. REMOVE BRAKE ACTUATOR ASSEMBLY WITH BRACKET

1. Place tags or marks to identify the installation locations of each brake line.

1. Release the latch of the actuator connector and disconnect the connector.

1. Using SST, disconnect the 5 brake lines from the actuator.

   SST
     09023-00101

1. LHD:
   Remove the 3 bolts and actuator with bracket.

1. RHD:
   Remove the 3 nuts and actuator with bracket.

   NOTICE:
     Be careful not to damage the brake tubes.