GSIC - Global Service Information Center

# HEATED OXYGEN SENSOR (for Sensor 2) > ON-VEHICLE INSPECTION

## for Preparation Click here

1. INSPECT HEATED OXYGEN SENSOR

1. Using an ohmmeter, measure the resistance between the terminals.

   Standard resistance:

     Tester Connection | Specified Condition
     1 (HT) - 2 (+B) | 11 to 16 Ω at 20°C (68°F)
     1 (HT) - 4 (E1) | 10 kΩ or higher

   If the resistance is not as specified, replace the sensor.