GSIC - Global Service Information Center

# BRAKE MASTER CYLINDER > REMOVAL

## for Preparation Click here

1. DRAIN BRAKE FLUID

NOTICE:

  Wash off brake fluid immediately if it comes in contact with any painted surface.

2. REMOVE BRAKE MASTER CYLINDER SUB-ASSEMBLY (w/o ABS)

1. M/T:
   Disconnect the clutch reservoir tube labeled A from the master cylinder.

1. Disconnect the brake fluid warning switch connector labeled B.

1. Using SST, disconnect the 6 brake lines labeled C from the master cylinder and 4-way.

   SST
     09023-00101

1. Remove the 2 nuts and bracket (with 4-way).

1. Pull out the master cylinder from the brake booster.

1. Remove the O-ring from the master cylinder.

3. REMOVE BRAKE MASTER CYLINDER SUB-ASSEMBLY (w/ ABS)

1. M/T:
   Disconnect the clutch reservoir tube labeled A from the master cylinder.

1. Disconnect the brake fluid level warning switch connector labeled B.

1. Using SST, disconnect the 5 brake lines labeled C from the master cylinder and 3-way.

   SST
     09023-00101

1. Remove the 2 nuts and bracket (with 3-way).

1. Pull out the master cylinder from the brake booster.

1. Remove the O-ring from the master cylinder.

4. REMOVE BRAKE MASTER CYLINDER RESERVOIR SUB-ASSEMBLY

1. Remove the screw.

1. Remove the reservoir and 2 grommets from the master cylinder.