GSIC - Global Service Information Center

# REAR BUMPER (for Flat Type) > REASSEMBLY

## for Preparation Click here

1. INSTALL REAR BUMPER BAR PLATE

1. Clean the bumper bar surface.

   1. Using a heat light, heat the bumper bar surface.

      Standard:

        Item | Heating temperature
        Rear bumper bar | 40 to 60°C (104 to 140°F)

      NOTICE:
        Do not heat the bumper bar excessively.

   2. Remove the double-sided tape from the bumper bar.

   3. Wipe off any tape adhesive residue with cleaner.

1. If reusing the bumper bar plate:
   Clean the bumper bar plate.

   1. Using a heat light, heat the bumper bar plate.

      Standard:

        Item | Heating temperature
        Rear bumper bar plate | 20 to 30°C (68 to 86°F)

      NOTICE:
        Do not heat the bumper bar plate excessively.

   2. Remove the double-sided tape from the bumper bar plate.

   3. Wipe off any tape adhesive residue with cleaner.

   4. Apply new double-sided tape to the bumper bar plate as shown in the illustration.

      Specification:

        Area | Measurement
        a | 15.0 mm (0.591 in.)
        b | 85.0 mm (3.346 in.)
        c | 4.0 mm (0.157 in.)
        d | 7.0 mm (0.276 in.)
        e | 1.2 mm (0.047 in.)
        f | 3.0 mm (0.118 in.)

   5. Install the bumper bar plate to the bumper bar.

2. INSTALL REAR BUMPER PLATE LH

1. Attach the 2 claws to install the bumper plate.

3. INSTALL REAR BUMPER PLATE RH

HINT:

  Use the same procedures described for the LH side.

4. INSTALL REAR BUMPER PLATE

1. Attach the 13 claws to install the bumper plate.

5. INSTALL LICENSE PLATE LIGHT ASSEMBLY

1. Attach the 4 claws to install the 2 lights.