GSIC - Global Service Information Center

### FRONT WIPER MOTOR AND LINK > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE FRONT WIPER ARM HEAD CAP

3. REMOVE FRONT WIPER ARM & BLADE ASSEMBLY LH

4. REMOVE FRONT WIPER ARM & BLADE ASSEMBLY RH

5. REMOVE HOOD TO COWL TOP SEAL

6. REMOVE COWL TOP VENTILATOR LOUVER LH

7. REMOVE COWL TOP VENTILATOR LOUVER RH

8. REMOVE WINDSHIELD WIPER MOTOR & LINK ASSEMBLY

9. REMOVE WINDSHIELD WIPER MOTOR ASSEMBLY