GSIC - Global Service Information Center

### PARKING BRAKE CABLE (for 4WD) > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE REAR WHEEL

3. REMOVE REAR BRAKE DRUM SUB-ASSEMBLY

4. REMOVE SHIFT LEVER KNOB SUB-ASSEMBLY

5. REMOVE PARKING BRAKE HOLE COVER SUB-ASSEMBLY

6. REMOVE UPPER CONSOLE PANEL PANEL SUB-ASSEMBLY

7. REMOVE CONSOLE BOX ASSEMBLY

8. REMOVE NO. 1 PARKING BRAKE CABLE ASSEMBLY

9. REMOVE NO. 2 PARKING BRAKE CABLE ASSEMBLY

10. REMOVE NO. 3 PARKING BRAKE CABLE ASSEMBLY