GSIC - Global Service Information Center

# AIR CONDITIONING AND BLOWER UNIT > INSTALLATION

## for Preparation Click here

1. INSTALL AIR CONDITIONING AND BLOWER ASSEMBLY

1. Install the A/C unit with the bolt and nut.

   Torque:
     9.8 N*m{ 100 kgf*cm , 7 ft.*lbf }

2. INSTALL INSTRUMENT PANEL REINFORCEMENT

1. Install the instrument panel reinforcement with the 7 bolts.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf } for bolt A
     18 N*m{ 184 kgf*cm , 13 ft.*lbf } for bolt B

1. Install the 3 bolts.

   Torque:
     9.8 N*m{ 100 kgf*cm , 7 ft.*lbf }

1. Install the 12 clamps.

1. Connect the connectors.

1. Install the grommet.

1. Install the ground wires with the 2 bolts to the instrument panel reinforcement.

1. Connect the connector, 3 clamps and wire harness.

1. Attach the clamp to the A/C unit.

3. INSTALL ECM

1. Install the ECM with the bolt and 2 nuts.

   Torque:
     12.5 N*m{ 128 kgf*cm , 9 ft.*lbf }

1. Connect the 4 connectors.

4. INSTALL STEERING COLUMN ASSEMBLY

1. Install the steering column with the 3 bolts.

   Torque:
     21 N*m{ 214 kgf*cm , 15 ft.*lbf }

5. INSTALL NO. 1 COOLER UNIT DRAIN HOSE

1. Install the drain hose.

6. INSTALL NO. 1 INSTRUMENT PANEL BRACE SUB-ASSEMBLY

1. Install the 3 nuts , 2 bolts, 2 clamps and instrument panel brace.

1. Connect the connectors and install the instrument panel junction block.

7. INSTALL NO. 3 HEATER TO REGISTER DUCT

1. Attach the 4 claws and install the duct.

8. INSTALL NO. 1 HEATER TO REGISTER DUCT

1. Attach the 3 claws and install the duct.

9. INSTALL NO. 2 HEATER TO REGISTER DUCT

1. Install the duct with the clip.

10. INSTALL INSTRUMENT PANEL SUB-ASSEMBLY LOWER

1. Install the instrument panel sub-assembly lower (Click here).

11. INSTALL INSTRUMENT PANEL SUB-ASSEMBLY UPPER

1. Install the instrument panel sub-assembly upper (Click here).

12. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

13. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

14. CHECK SRS WARNING LIGHT

1. Check the SRS warning light (Click here).