GSIC - Global Service Information Center

# POWER MIRROR CONTROL SYSTEM > INSPECTION

## for Preparation Click here

1. INSPECT OUTER MIRROR SWITCH ASSEMBLY

1. The L position of the left/right adjustment switch: Measure the resistance of the mirror switch.

   Standard (Left side):

     Tester Connection | Switch Condition | Specified Condition
     4 (MLV) - 8 (B) 6 (M+) - 7 (E) | UP | Below 1 Ω
     4 (MLV) - 7 (E) 6 (M+) - 8 (B) | DOWN | Below 1 Ω
     5 (MLH) - 8 (B) 6 (M+) - 7 (E) | LEFT | Below 1 Ω
     5 (MLH) - 7 (E) 6 (M+) - 8 (B) | RIGHT | Below 1 Ω

   If the result is not as specified, replace the switch assembly.

1. The R position of the left/right adjustment switch: Measure the resistance of the mirror switch.

   Standard (Right side):

     Tester Connection | Switch Condition | Specified Condition
     3 (MRV) - 8 (B) 6 (M+) - 7 (E) | UP | Below 1 Ω
     3 (MRV) - 7 (E) 6 (M+) - 8 (B) | DOWN | Below 1 Ω
     2 (MRH) - 8 (B) 6 (M+) - 7 (E) | LEFT | Below 1 Ω
     2 (MRH) - 7 (E) 6 (M+) - 8 (B) | RIGHT | Below 1 Ω

   If the result is not as specified, replace the switch assembly.

2. INSPECT OUTER REAR VIEW MIRROR ASSEMBLY LH

1. Disconnect the mirror connector.

1. Apply battery voltage and check operation of the mirror.

   OK:

     Measurement Condition | Specified Condition
     Battery positive (+) →Terminal 5 (MV) Battery negative (-) → Terminal 3 (M+) | Turns upward (A)
     Battery positive (+) → Terminal 3 (M+) Battery negative (-) → Terminal 5 (MV) | Turns downward (B)
     Battery positive (+) → Terminal 1 (MH) Battery negative (-) → Terminal 3 (M+) | Turns left (C)
     Battery positive (+) → Terminal 3 (M+) Battery negative (-) → Terminal 1 (MH) | Turns right (D)

   If the result is not as specified, replace the mirror assembly.

3. INSPECT OUTER REAR VIEW MIRROR ASSEMBLY RH

1. Disconnect the mirror connector.

1. Apply battery voltage and check operation of the mirror.

   OK:

     Measurement Condition | Specified Condition
     Battery positive (+) → Terminal 5 (MV) Battery negative (-) → Terminal 3 (M+) | Turns upward (A)
     Battery positive (+) → Terminal 3 (M+) Battery negative (-) → Terminal 5 (MV) | Turns downward (B)
     Battery positive (+) → Terminal 1 (MH) Battery negative (-) → Terminal 3 (M+) | Turns left (C)
     Battery positive (+) → Terminal 3 (M+) Battery negative (-) → Terminal 1 (MH) | Turns right (D)

   If the result is not as specified, replace the mirror assembly.