GSIC - Global Service Information Center

# GLOW PLUG > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag activation

2. REMOVE NO. 2 AIR CLEANER PIPE SUB-ASSEMBLY

1. Disconnect the manifold absolute pressure sensor connector.

1. Disconnect the vacuum hose from the gas filter.

1. Loosen the 2 clamps.

1. Remove the bolt and disconnect the pipe together with the 2 air hoses.

3. REMOVE VACUUM SWITCHING VALVE BRACKET

1. Remove the 2 bolts and bracket.

4. REMOVE DIESEL THROTTLE BODY ASSEMBLY

1. Disconnect the 2 connectors.

1. Remove the 2 bolts, 2 nuts, throttle body and gasket.

5. REMOVE THROTTLE BODY BRACKET

1. Remove the 3 bolts and bracket.

6. REMOVE INTAKE AIR CONNECTOR

1. Remove the 2 nuts, bolt, air connector and bracket.

7. REMOVE NO. 1 GLOW PLUG CONNECTOR

1. Remove the nut and wire harness.

1. Remove the 4 screw grommets, 4 nuts and glow plug connector.

8. REMOVE GLOW PLUG ASSEMBLY

1. Using a 12 mm deep socket wrench, remove the 4 glow plugs.