GSIC - Global Service Information Center

### STEERING COLUMN ASSEMBLY > DISASSEMBLY

1. REMOVE STEERING SLIDING WITH COUPLING YOKE SUB-ASSEMBLY

2. REMOVE NO.2 STEERING INTERMEDIATE SHAFT SUB-ASSEMBLY

3. INSPECT STEERING COLUMN ASSY

4. REMOVE TRANSPONDER KEY AMPLIFIER

5. REMOVE STEERING COLUMN UPPER WITH SWITCH BRACKET ASSEMBLY

6. REMOVE STEERING COLUMN UPPER CLAMP

7. REMOVE IGNITION SWITCH LOCK CYLINDER ASSEMBLY

8. REMOVE UNLOCK WARNING SWITCH ASSEMBLY

9. REMOVE IGNITION OR STARTER SWITCH ASSEMBLY

10. REMOVE KEY INTER LOCK SOLENOID

11. REMOVE STEERING MAIN SHAFT ASSEMBLY