GSIC - Global Service Information Center

# FRONT NO. 1 SPEAKER > INSTALLATION

## for Preparation Click here

HINT:

1. Use the same procedures for the RH side and LH side.
2. The procedures listed below are for the LH side.

1. INSTALL FRONT NO. 1 SPEAKER ASSEMBLY

1. Install the speaker to the door.

1. Using an air riveter or hand riveter, install the speaker with 3 new rivets.

   NOTICE:

   1. Do not pry the rivet with the riveter, as this will cause damage to the riveter and mandrel.

   2. Confirm that the rivets are seated properly against the speaker.
      Do not tilt the riveter when installing the rivet to the speaker.
      Do not leave any space between the rivet head and speaker.

   3. Do not leave any space between the speaker and door. Firmly hold together the 2 items while installing the rivet.

1. Connect the connector.

2. INSTALL FRONT DOOR TRIM BOARD SUB-ASSEMBLY

1. Remove the screw labeled A and clip labeled B.

1. Remove the trim.

   1. Double cab:
      Using a screwdriver, detach the 8 remaining clips and remove the trim.

   2. Single cab:
      Using a screwdriver, detach the 9 remaining clips and remove the trim.

      HINT:
      1. Tape the screwdriver tip before use.
      2. If the screwdriver cannot reach the clips, pull on the lower trim to remove it.

      NOTICE:
      1. The clip labeled C cannot be reused. When installing the trim board, replace clip C.
      2. In order to prevent the door panel from being damaged, use protective tape to cover the areas indicated by the arrows in the illustration.

1. Using a screwdriver, detach the 7 claws and remove the weatherstrip inner.

   HINT:
     Tape the screwdriver tip before use.

3. INSTALL FRONT ARMREST BASE PANEL UPPER LH (w/ Power Window)

1. Passenger side:
   Attach the 2 claws and install the window regulator switch to the base panel.

1. Driver side:

   1. Install the window regulator master switch to the base panel.

   2. Install the 3 screws.

1. Connect the switch connector.

1. Attach the clip and 5 claws to install the panel together with the window regulator master switch.

4. INSTALL DOOR PULL HANDLE

1. Install the screw and pull handle.

5. INSTALL FRONT DOOR LOWER FRAME BRACKET GARNISH LH

1. Attach the 2 clips to install the garnish.

6. INSTALL FRONT DOOR WINDOW REGULATOR HANDLE ASSEMBLY (w/o Power Window)

1. Install the snap ring to the regulator handle.

1. With the window fully closed, install the regulator handle and plate to the regulator shaft, as shown in the illustration.

7. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

8. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.