GSIC - Global Service Information Center

# SUSPENSION > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
FRONT |
Hub nut | 2WD | Steel wheel | 152 | 1,550 | 112
Aluminum wheel | 121 | 1,234 | 89
4WD | 105 | 1,071 | 77
Tie rod end lock nut | 55.5 | 566 | 41
Suspension support x Piston rod | 18 | 184 | 13
Stabilizer bar link x Lower arm | 78 | 795 | 58
Stabilizer bracket x Body | 48 | 489 | 35
Stabilizer bar x Stabilizer link | 70 | 714 | 52
Shock absorber with coil spring x Lower arm | 95 | 969 | 70
Shock absorber with coil spring x Body | 40 | 408 | 30
Upper arm x Axle | 85 | 867 | 63
Upper arm x Lower arm | 110 | 1,122 | 81
Skid control sensor wire x Body | 29 | 296 | 21
Lower suspension arm set nut | 210 | 2,141 | 155
Lower ball joint attachment x Lower arm | 140 | 1,428 | 103
Lower ball joint attachment x Steering knuckle | 160 | 1,632 | 118
REAR |
Hub nut | 2WD | Steel wheel | 152 | 1,550 | 112
Aluminum wheel | 121 | 1,234 | 89
4WD | 105 | 1,071 | 77
Shock absorber x Spring seat | 105 | 1,070 | 77
Shock absorber x Frame | 105 | 1,070 | 77
U-bolt x Spring seat | 120 | 1,224 | 89
Rear spring pin set bolt x Frame | Single cab | 32 | 326 | 24
Rear spring bracket pin x Leaf spring | Single cab | 120 | 1,224 | 89
Rear spring pin bolt x Leaf spring | Extra, double cab | 120 | 1,224 | 89
Rear spring shackle x Leaf spring | 60 | 612 | 44