GSIC - Global Service Information Center

# VACUUM REGULATING VALVE > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE NO. 1 ENGINE COVER SUB-ASSEMBLY

1. Remove the 3 bolts, 2 nuts and cover.

3. REMOVE VACUUM SWITCHING VALVE BRACKET

1. Disconnect the 2 connectors.

1. Disconnect the vacuum hoses from the 3 locations.

1. Remove the 2 bolts and bracket.

4. REMOVE VACUUM SWITCHING VALVE (for EGR CUT)

1. Remove the bolt and valve.