GSIC - Global Service Information Center

# EXTENSION HOUSING REAR OIL SEAL > INSTALLATION

## for Preparation Click here

1. INSTALL AUTOMATIC TRANSMISSION EXTENSION HOUSING OIL SEAL

1. Coat the lip of the oil seal with MP grease.

1. Using SST and a hammer, carefully tap in a new oil seal in as far as possible.

   SST
     09316-60011 (09316-00011, 09316-00051)

   Oil seal depth from flat end:
     5.4 to 5.8 mm (0.213 to 0.228 in.)

2. INSTALL PROPELLER SHAFT WITH CENTER BEARING ASSEMBLY

1. Install the propeller shaft with center bearing assembly (Click here).

3. ADD AUTOMATIC TRANSMISSION FLUID

1. Add automatic transmission fluid (Click here).

4. INSPECT AUTOMATIC TRANSMISSION FLUID

1. Inspect the automatic transmission fluid (Click here).