GSIC - Global Service Information Center

# FUEL TEMPERATURE SENSOR > INSTALLATION

## for Preparation Click here

1. INSTALL FUEL TEMPERATURE SENSOR

1. Using a 19 mm deep socket wrench, install the sensor.

   Torque:
     N*m{ kgf*cm , ft.*lbf }

1. Connect the connector.

2. ADD FUEL

3. BLEED AIR FROM FUEL SYSTEM

1. Using the hand pump, bleed air from the fuel system until pumping becomes difficult.

4. CONNECT BATTERY TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

6. CHECK FOR FUEL LEAKS