GSIC - Global Service Information Center

# 1TR-FE ENGINE CONTROL SYSTEM > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Throttle body assembly x Intake manifold | 9.0 | 92 | 80 in.*lbf
Intake manifold assembly x Cylinder head | 25 | 255 | 18
Knock sensor x Cylinder block | 20 | 204 | 15
Accelerator pedal rod assembly x Body | 7.5 | 76 | 66 in.*lbf
ECM x Instrument panel reinforcement | 12.5 | 127 | 9
ECM x Blower assembly | 12.5 | 127 | 9
ECM x ECM bracket | 3.0 | 31 | 27 in.*lbf
Camshaft timing oil control valve assembly x Cylinder head | 8.5 | 87 | 75 in.*lbf
Camshaft position sensor x Cylinder head | 8.5 | 87 | 75 in.*lbf
Crankshaft position sensor x Cylinder block | 8.5 | 87 | 75 in.*lbf
Starter assembly x Transmission | 37 | 377 | 27