GSIC - Global Service Information Center

### FUEL TANK > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. LOOSEN FUEL TANK CAP

3. REMOVE NO. 1 FUEL TANK PROTECTOR

4. DISCONNECT FUEL MAIN TUBE AND FUEL RETURN TUBE

5. DISCONNECT FUEL TANK TO FILLER PIPE HOSE

6. DISCONNECT FUEL TANK BREATHER HOSE

7. REMOVE FUEL TANK FILLER PIPE

8. REMOVE FUEL TANK

9. REMOVE NO. 1 FUEL TANK CUSHION

10. REMOVE FUEL PUMP GAUGE RETAINER

11. REMOVE FUEL SUCTION WITH PUMP AND GAUGE TUBE ASSEMBLY