GSIC - Global Service Information Center

# FRONT SUSPENSION UPPER ARM (for 4WD) > INSTALLATION

## for Preparation Click here

1. TEMPORARILY INSTALL FRONT SUSPENSION UPPER ARM ASSEMBLY LH

1. Temporarily install the upper arm with the bolt, 2 retainers and nut.

   HINT:
     Fix the nut in place and temporarily install the bolt.

1. Install the upper arm to the steering knuckle with a nut.

   Torque:
     110 N*m{ 1,122 kgf*cm , 81 ft.*lbf }

1. Install a new clip.

2. CONNECT SKID CONTROL SENSOR WIRE

1. Install the sensor wire with the 2 bolts.

   Torque:
     29 N*m{ 296 kgf*cm , 21 ft.*lbf }

3. INSTALL FRONT WHEEL

1. Install the front wheel.

   Torque:
     105 N*m{ 1,071 kgf*cm , 77 ft.*lbf }

4. STABILIZE SUSPENSION

1. Lower the vehicle.

1. Press down on the vehicle several times to stabilize the suspension.

5. TIGHTEN FRONT SUSPENSION UPPER ARM ASSEMBLY

1. Tighten the upper arm's bolt.

   Torque:
     115 N*m{ 1,173 kgf*cm , 85 ft.*lbf }

   NOTICE:
     Do not tighten the nut.

6. INSPECT AND ADJUST FRONT WHEEL ALIGNMENT

Inspect and adjust the front wheel alignment (Click here).