GSIC - Global Service Information Center

### FRONT SEAT INNER BELT ASSEMBLY > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE FRONT SEAT ASSEMBLY (for Separate Seat Type)

3. REMOVE FRONT SEAT ASSEMBLY (for Bench Seat Type)

4. REMOVE FRONT SEAT INNER BELT ASSEMBLY

5. REMOVE FRONT SEAT INNER BELT ASSEMBLY (for Separate Seat Type)

6. REMOVE FRONT SEAT INNER W/ CENTER BELT ASSEMBLY RH (for Bench Seat Type)

7. REMOVE FRONT SEAT INNER W/ CENTER BELT ASSEMBLY LH (for Bench Seat Type)