GSIC - Global Service Information Center

# HOOD LOCK CONTROL CABLE ASSEMBLY > INSTALLATION

## for Preparation Click here

1. INSTALL HOOD LOCK CONTROL CABLE ASSY

1. Install the cable to the clamps as shown in the illustration.

1. Install the grommet to the vehicle body.

1. Install the open lever.

2. INSTALL HOOD LOCK ASSEMBLY

1. Connect the cable to the lock.

1. Install the lock with the 3 bolts.

   Torque:
     8.0 N*m{ 82 kgf*cm , 71 in.*lbf }

1. Adjust the lock.

1. w/ Hood courtesy switch:
   Connect the connector and attach the clamp.

3. INSTALL RADIATOR GRILLE

1. Push the radiator grille in the direction indicated by the arrow in the illustration. Attach the 5 claws to install the radiator grille.

1. Install the 2 screws and 2 clips.

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.