GSIC - Global Service Information Center

# INJECTOR DRIVER > INSTALLATION

## for Preparation Click here

1. INSTALL INJECTOR DRIVER BRACKET

1. Install the driver bracket with the 3 screws.

   Torque:
     2.0 N*m{ 20 kgf*cm , 18 in.*lbf }

2. INSTALL INJECTOR DRIVER

1. Install the injector driver with the 2 bolts.

1. Connect the 2 connectors.

   Torque:
     12.5 N*m{ 128 kgf*cm , 9 ft.*lbf }

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

5. READ REGISTERED DATA

1. Read the registered data (see page ).