GSIC - Global Service Information Center

### RADIATOR > INSTALLATION

1. INSTALL RADIATOR ASSEMBLY

2. CONNECT NO. 1 OIL COOLER TUBE INLET (for Automatic Transmission)

3. CONNECT NO. 1 OIL COOLER TUBE OUTLET (for Automatic Transmission)

4. INSTALL FAN SHROUD

5. INSTALL AIR PUMP INLET (for Unleaded Gasoline Specification Vehicle)

6. CONNECT RADIATOR HOSE INLET

7. CONNECT RADIATOR HOSE OUTLET

8. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

9. ADD ENGINE COOLANT

10. CHECK FOR ENGINE COOLANT LEAKS

11. INSTALL RADIATOR SIDE DEFLECTOR LH

12. INSTALL RADIATOR SIDE DEFLECTOR RH

13. INSTALL RADIATOR GRILLE

14. INSTALL NO. 1 ENGINE UNDER COVER

15. PERFORM INITIALIZATION