GSIC - Global Service Information Center

# FUEL FILTER > INSTALLATION

## for Preparation Click here

1. INSTALL FUEL FILTER

1. Install the fuel filter with the 3 nuts.

   Torque:
     8.5 N*m{ 87 kgf*cm , 75 in.*lbf }

1. Connect the charcoal canister.

2. CONNECT FUEL MAIN TUBE

NOTICE:

  Before installing the fuel main tube's connector to the fuel filter's upper pipe, check the connector for damage and foreign matter.

1. Connect the connector to the upper pipe. Push the two parts together firmly until a "click" sound is heard. Then attach the lock claws to the connector by pushing down on the connector cover.

1. Check that the connector and upper pipe are securely connected by trying to pull them apart.

1. Install the fuel tube grommet.

3. CONNECT FUEL HOSE

1. Connect the connector to the lower pipe. Push the two parts together firmly until a "click" sound is heard.

1. Check that the connector and lower pipe are securely connected by trying to pull them apart.

1. Connect the hose to the clamp.

4. INSTALL CHARCOAL CANISTER (for Unleaded Gasoline Specification Vehicle)

1. Attach the canister to the stay.

1. Connect the 3 hoses to the canister.

5. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

6. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

7. CHECK FOR FUEL LEAKS

1. Connect the intelligent tester to the DLC3.

   1. Turn the ignition switch ON.

      NOTICE:
        Do not start the engine.

   2. Push the intelligent tester main switch ON.

   3. Select the Active Test and enter the following menus: Powertrain / Engine and ECT / Active Test / Control the Fuel Pump / Speed.

1. Check for fuel leaks.

   1. Check that there are no fuel leaks after performing maintenance anywhere on the fuel system.