GSIC - Global Service Information Center

# REAR BRAKE (for 2WD) > DISASSEMBLY

## for Preparation Click here

HINT:

1. Use the same procedures for the LH side and RH side.
2. The procedures listed below are for the LH side.

1. DISCONNECT REAR BRAKE SHOE RETURN SPRING

1. Using SST, disconnect the spring from the front brake shoe and rear brake shoe.

   SST
     09703-30011

   NOTICE:
     Be careful not to damage the wheel cylinder boot.

2. REMOVE FRONT BRAKE SHOE

1. Using SST, remove the shoe hold down spring cup, shoe hold down spring and pin.

   SST
     09718-00010

1. Remove the shoe and tension spring.

3. REMOVE PARKING BRAKE SHOE STRUT SET LH

1. Remove the strut set from the rear brake shoe.

4. REMOVE REAR BRAKE SHOE

1. Using SST, remove the shoe hold down spring cup, shoe hold down spring and pin.

   SST
     09718-00010

1. Using needle-nose pliers, remove the adjust lever tension spring from the automatic adjust lever. Then remove the shoe.

1. Using needle-nose pliers, disconnect the No. 3 parking brake cable from the parking brake shoe lever.

5. REMOVE REAR BRAKE AUTOMATIC ADJUST LEVER LH

1. Using a screwdriver, remove the E-ring and lever.

6. REMOVE REAR BRAKE PARKING BRAKE SHOE LEVER SUB-ASSEMBLY

1. Using a screwdriver, remove the C-washer and lever.

7. REMOVE REAR WHEEL BRAKE CYLINDER ASSEMBLY LH

1. Using SST, disconnect the brake line.

   SST
     09023-00101

1. Remove the 2 bolts and cylinder.

8. REMOVE REAR WHEEL BRAKE CYLINDER CUP

1. Remove the 2 cylinder dust boots from the cylinder.

1. Remove the 2 pistons and compression spring.

1. Remove the 2 cups from each piston.

9. REMOVE REAR BRAKE DRUM BLEEDER PLUG

1. Remove the bleeder plug cap and bleeder plug from the cylinder.