GSIC - Global Service Information Center

# AIR SWITCHING VALVE (for Unleaded Gasoline Specification Vehicle) > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE AIR CLEANER ASSEMBLY

1. Disconnect the MAF meter connector.

1. Loosen the hose clamp.

1. Remove the 2 bolts and air cleaner.

3. DISCONNECT NO. 4 AIR HOSE

1. Loosen the clamp and disconnect the No. 4 hose.

4. REMOVE NO. 1 EXHAUST MANIFOLD HEAT INSULATOR

1. Remove the 5 bolts and heat insulator.

5. REMOVE INTAKE PIPE INSULATOR

1. Remove the 4 nuts, pipe and 2 gaskets.

6. REMOVE AIR SWITCHING VALVE ASSEMBLY

1. Disconnect the connector.

1. Remove the 2 nuts and switching valve.