GSIC - Global Service Information Center

# MANUAL TRANSMISSION EXTENSION HOUSING OIL SEAL > INSTALLATION

## for Preparation Click here

1. INSTALL MANUAL TRANSMISSION EXTENSION HOUSING OIL SEAL

1. Coast the lip of a new oil seal with MP grease.

1. Using SST and a hammer, tap in the oil seal.

   SST
     09223-00010

   Oil seal depth:
     0 +- 0.5 mm (0 +- 0.020 in.)

   NOTICE:
     Be careful not to damage the lip of the oil seal.

2. INSTALL MANUAL TRANSMISSION UNIT ASSEMBLY

1. Install the manual transmission unit assembly (Click here).