GSIC - Global Service Information Center

### FUEL TANK > REMOVAL

1. DISCHARGE FUEL SYSTEM PRESSURE

2. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

3. REMOVE FUEL TANK CAP

4. REMOVE NO. 3 FUEL TUBE CLAMP

5. DISCONNECT FUEL MAIN TUBE AND FUEL RETURN TUBE

6. DISCONNECT FUEL TANK TO FILLER PIPE HOSE

7. DISCONNECT FUEL TANK BREATHER HOSE

8. REMOVE FUEL TANK FILLER PIPE

9. REMOVE FUEL TANK

10. REMOVE NO. 1 FUEL TANK CUSHION

11. REMOVE FUEL PUMP GAUGE RETAINER

12. REMOVE FUEL SUCTION WITH PUMP AND GAUGE TUBE ASSEMBLY