GSIC - Global Service Information Center

# IGNITION COIL > INSTALLATION

## for Preparation Click here

1. INSTALL IGNITION COIL

1. Connect a new ignition coil to the spark plug, attach the ignition coil to the cylinder head cover, and install the bolt.

   Torque:
     7.5 N*m{ 76 kgf*cm , 66 in.*lbf }

1. Connect the ignition coil connector.

2. INSTALL INTAKE AIR CONNECTOR

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.