GSIC - Global Service Information Center

# 1TR-FE EMISSION CONTROL > TORQUE SPECIFICATIONS

Vacuum switching valve (for EVAP):

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Vacuum switching valve x Intake manifold | 9.0 | 92 | 80 in.*lbf

Ventilation valve sub-assembly:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Ventilation valve sub-assembly x Cylinder head cover | 5.0 | 51 | 44 in.*lbf

Heated oxygen sensor:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Heated oxygen sensor x Front exhaust pipe assembly | For use with SST | 40 | 408 | 30
  For use without SST | 44 | 449 | 32